Open Book/Notes quiz

**1)** **(5 points)** What addressing mode is being used by the following instruction?

mov.w R4,R5

Register

**2) (5 points)** What addressing mode is being used by the following instruction?

mov.w #0xFF11h,R5

Immediate

**3) (5 points)** After execution of the instruction from question 2, mov.w #0xFF11h, what value will be in register R5.

$FF11 or 0xFF11h

**4) (5 points)** The & is used to indicate which addressing mode?

Absolute